Timing of TIM Output Signals ^{JBL/TJF}_{UCL}^{8/8/99}_{7/9/99}

BC BCR L1A Serial ID Serial TT

Calibration Command: CAL L1A

Not to scale setup

offset BCID-offset

1 - 10 s

0 - 7 s

LSB first 1 0 1 0 24-bit L1ID + 12-bit BCID

TYPE (8+2 bits) (assuming < 8 L1As in 80 s)μ μ μ

pipeline length = 132 BCs

3 bits 27 bits