R.L. Wastie 01/09/97

Biphase Mark LED Driver

Biphase Mark Encoder

Fine Delay 500ps steps 128 steps

Data Cycle Delay 32 Cycles

Data IN

Cycle Delay Select LED Driver

Drive Strength

Edge Slew Rate

VDD

Fine Delay Select

Fine Delay 500ps steps 128 steps

80Mhz CLOCK

40Mhz CLOCK