{"text_format":"5","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"props":{"creator":"Matthew Warren","last_modified_by":"Matthew Warren","company":"UCL"},"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":132,"n_cols":9,"rows_kept":132,"flags":["formulas_cached_only"]}
["TIM SIGNALS:",null,null,"Old - TIM2",null,"New"]
["PLD","IO","NAME","Old Source/Destination","Old Source/Destination","Int or Ext","TIM, Mgr, Other","New Source/ Destination","New Source/Destination"]
["new","BIPUT","db[31..0]","-","-","e","m","v","VME"]
["new","BIPUT","DebugBus[15..0]","-","-","e","mt","dbh","Debug Bus Header"]
["new","BIPUT","DebugBus[15..0]","-","-","e","t","dbh","Debug Bus Header"]
["new","BIPUT","SpareBus[7..0]","-","-","e","mt","tim","TIM"]
["new","BIPUT","TCROM_data","-","-","e","m","crt","Config EEPROM (TIM)"]
["new","BIPUT","TCROM_data","-","-","e","t","crt","Config EEPROM (TIM)"]
["new","INPUT","ab[31..1]","-","-","e","m","v","VME"]
["new","INPUT","DebugMode[3..0]","-","-","e","m","dms","Debug Mode Switch"]
["new","INPUT","DebugMode[3..0]","-","-","e","t","dms","Debug Mode Switch"]
["new","INPUT","ExtClkOff","-","-","e","t","cc","Clock Control"]
["new","INPUT","IntClkOff","-","-","e","t","cc","Clock Control"]
["new","INPUT","MCROM_data","-","-","e","m","crm","Config EEPROM (Mgr)"]
["new","INPUT","PO_reset","-","-","e","m","por","Power-On Reset"]
["new","INPUT","SAClkOff","-","-","e","t","cc","Clock Control"]
["new","INPUT","TCROM_ready","-","-","e","m","crt","Config EEPROM (TIM)"]
["new","INPUT","TIM_ID[7..0]","-","-","e","m","ti","TIM ID"]
["new","INPUT","TIM_ID[7..0]","-","-","e","t","ti","TIM ID"]
["new","INPUT","TIMselect","-","-","e","mt","tim","TIM"]
["new","INPUT","TTCClkOff","-","-","e","t","cc","Clock Control"]
["new","OUTPUT","enIntClk","-","-","e","t","cc","Clock Control"]
["new","OUTPUT","enSAClk","-","-","e","t","cc","Clock Control"]
["new","OUTPUT","FPGA2_nprog","-","-","e","m","trp","TIM Reset/Prog System"]
["new","OUTPUT","TCROM_clk","-","-","e","m","crt","Config EEPROM (TIM)"]
["new","OUTPUT","TCROM_nce","-","-","e","m","crt","Config EEPROM (TIM)"]
["new","OUTPUT","TCROM_nser_en","-","-","e","m","crt","Config EEPROM (TIM)"]
["new","OUTPUT","TCROM_rst_noe","-","-","e","m","crt","Config EEPROM (TIM)"]
["new","OUTPUT","TCROM_wp1","-","-","e","m","crt","Config EEPROM (TIM)"]
["new","OUTPUT","TCROM_wp2","-","-","e","m","crt","Config EEPROM (TIM)"]
["pld1","INPUT","amb[5..0]","v","VME","e","m","v","VME"]
["pld1","INPUT","B_select","j","Jumpers & DIPs","e","m","j","Jumpers & DIPs"]
["pld1","INPUT","base_addr[31..16]","ba","Base Addr. Switches","e","m","v","VME"]
["pld1","INPUT","BaseAddr_Select","j","Jumpers & DIPs","e","m","v","VME"]
["pld1","INPUT","dl1","dv","VME Delay Unit","e","m","dv","VME Delay Unit"]
["pld1","INPUT","dl2","dv","VME Delay Unit","e","m","dv","VME Delay Unit"]
["pld1","INPUT","dl3","dv","VME Delay Unit","e","m","dv","VME Delay Unit"]
["pld1","INPUT","nASb","v","VME","e","m","v","VME"]
["pld1","INPUT","nBErrb","v","VME","e","m","v","VME"]
["pld1","INPUT","nDS0b","v","VME","e","m","v","VME"]
["pld1","INPUT","nDS1b","v","VME","e","m","v","VME"]
["pld1","INPUT","nGAb[4..0]","v","VME","e","m","v","VME"]
["pld1","INPUT","nGAbp","v","VME","e","m","v","VME"]
["pld1","INPUT","nIAckb","v","VME","e","m","v","VME"]
["pld1","INPUT","nIAckinb","v","VME","e","m","v","VME"]
["pld1","INPUT","nLWordb","v","VME","e","m","v","VME"]
["pld1","INPUT","nWriteb","v","VME","e","m","v","VME"]
["pld1","OUTPUT","Ack","v","VME","e","m","v","VME"]
["pld1","OUTPUT","bRead","v","VME","e","mt","tim","TIM"]
["pld1","OUTPUT","bWrite","v","VME","e","mt","tim","TIM"]
["pld1","OUTPUT","dl0","dv","VME Delay Unit","e","m","dv","VME Delay Unit"]
["pld1","OUTPUT","nErrorLED","fl","Front-Panel LEDs","e","m","fl","Front-Panel LEDs"]
["pld1","OUTPUT","nGAoutEn","b","Back-Plane Signals","e","m","b","Back-Plane Signals"]
["pld1","OUTPUT","nIAckoutb","v","VME","e","m","v","VME"]
["pld1","OUTPUT","nIrqb[7..1]","v","VME","e","m","v","VME"]
["pld1","OUTPUT","nLE1","v","VME","e","m","v","VME"]
["pld1","OUTPUT","nLE2","v","VME","e","m","v","VME"]
["pld1","OUTPUT","nOEin","v","VME","e","m","v","VME"]
["pld1","OUTPUT","nOEout","v","VME","e","m","v","VME"]
["pld1","OUTPUT","nStop_Clk","cc","Clock Control","e","t","w","Trigger Window"]
["pld1","OUTPUT","Stop_Clk","cc","Clock Control","e","t","w","Trigger Window"]
["pld2","INPUT","extInBCREcl","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInBCRNim","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInCALEcl","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInCALNim","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInECREcl","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInECRNim","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInFEREcl","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInFERNim","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInSpareEcl","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInSpareNim","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInTRIGEcl","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","extInTRIGNim","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","intInECR","is","Internal Trig, FER, ECR","e","t","is","Internal Trig, FER, ECR"]
["pld2","INPUT","intInFER","is","Internal Trig, FER, ECR","e","t","is","Internal Trig, FER, ECR"]
["pld2","INPUT","intInTRIG","is","Internal Trig, FER, ECR","e","t","is","Internal Trig, FER, ECR"]
["pld2","INPUT","sReset","f","Front-Panel Signals","e","m","f","Front-Panel Signals"]
["pld2","INPUT","test_sw","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","INPUT","TRIG_win","w","Trigger Window","e","t","w","Trigger Window"]
["pld2","OUTPUT","CT[5..0]","cc","Clock Control","e","t","cc","Clock Control"]
["pld2","OUTPUT","enIntFER","is","Internal Trig, FER, ECR","e","t","is","Internal Trig, FER, ECR"]
["pld2","OUTPUT","enIntTRIG","is","Internal Trig, FER, ECR","e","t","is","Internal Trig, FER, ECR"]
["pld2","OUTPUT","enWindow","w","Trigger Window","e","t","w","Trigger Window"]
["pld2","OUTPUT","outTRIG","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld2","OUTPUT","SAMode","fl","Front-Panel LEDs","e","t","fl","Front-Panel LEDs"]
["pld2","OUTPUT","TIM_OK_out","b","Back-Plane Signals","e","t","b","Back-Plane Signals"]
["pld3","INPUT","laser_intlck_state","b","Back-Plane Signals","e","t","b","Back-Plane Signals"]
["pld3","OUTPUT","r[5..1]","is","Internal Trig, FER, ECR","e","t","is","Internal Trig, FER, ECR"]
["pld3","OUTPUT","s[5..1]","is","Internal Trig, FER, ECR","e","t","is","Internal Trig, FER, ECR"]
["pld3","OUTPUT","wd[5..0]","w","Trigger Window","e","t","w","Trigger Window"]
["pld3","OUTPUT","ws[5..0]","w","Trigger Window","e","t","w","Trigger Window"]
["pld6","OUTPUT","nTTCout[7..0]","b","Back-Plane Signals","e","t","b","Back-Plane Signals"]
["pld8","INPUT","extRodBusyIn","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld8","INPUT","nRodBusyb[21..5]","b","Back-Plane Signals","e","t","b","Back-Plane Signals"]
["pld8","OUTPUT","fp_rod_crate_busyout","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["pld8","OUTPUT","RBM[15..0]","rsv","Reserved","e","t","rsv","Reserved"]
["pld9","BIPUT","SCL","t","TTCrx","e","t","t","TTCrx"]
["pld9","BIPUT","SDA","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","BCnt[11..0]","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","BCntStr","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","Brcst[7..2]","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","BrcstStr1","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","BrcstStr2","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","DbErrStr","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","Dout[7..0]","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","DoutStr","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","DQ[3..0]","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","EvCntHStr","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","EvCntLStr","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","SinErrStr","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","SubAddr[7..0]","t","TTCrx","e","t","t","TTCrx"]
["pld9","INPUT","TTCReady","t","TTCrx","e","t","t","TTCrx"]
["pld9","OUTPUT","Resetb","t","TTCrx","e","t","t","TTCrx"]
["prim(all)","BIPUT","db[31..0]","v","VME","e","t","v","VME"]
["prim(all)","OUTPUT","nOA_rst","-","-","e","mt","tim","TIM"]
["prim(all)","OUTPUT","RunMode","fl","Front-Panel LEDs","e","t","fl","Front-Panel LEDs"]
["prim(pld1)","INPUT","ab[15..1]","v","VME","e","t","v","VME"]
["prim(pld9)","INPUT","BCRin","t","TTCrx","e","t","t","TTCrx"]
["prim(pld9)","INPUT","ECRin","t","TTCrx","e","t","t","TTCrx"]
["prim(pld9)","INPUT","L1Ain","t","TTCrx","e","t","t","TTCrx"]
["primary","INPUT","eclExtBusy","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","INPUT","NimExtBusy","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","BusyOut","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","eclBCR","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","eclCAL","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","eclECR","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","eclFER","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","eclID","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","eclL1A","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","eclSpare","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","eclTT","f","Front-Panel Signals","e","t","f","Front-Panel Signals"]
["primary","OUTPUT","rod_crate_BusyOut","fl","Front-Panel LEDs","e","t","fl","Front-Panel LEDs"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}