VCSEL Array Specifications

Characteristics Min. Typical Max. Units Wavelength 820 ~840 860 nm Output power coupled into 50mm core fibre @ 20mA

1 2 mW

Slope efficiency 60 100 mW/mA Absolute max. input power 35 mA Threshold current 3 6 mA Forward voltage @ 20mA 2 2.5 V Reverse voltage 2 V Rise/Fall time <1 2 ns Device reliability 500 FIT Temperature range 10 20 50 °C

Table 1: Technical specifications for the VCSEL arrays