Reverse dual 6 channel configuration - do not used this configuration ( because this loses the " Vout"s) always use the "standard dual 6"

VFE1 on bottom SCSI connector, link columns 3-2, 1-0, (top ADCs used, Vout connected to FPGA) VFE0 on top SCSI connector, link columns 8-7, 6-5, (bottom ADCs used, Vout connected to FPGA)