{"text_format":"5","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"props":{"creator":"wells","last_modified_by":"mp","company":"CERN"},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":87,"n_cols":9,"rows_kept":87,"flags":["formulas_cached_only"]}
["Summary of INEO spares"]
[]
["Notes: There was a mistake for sector 9 gap 29 barrel spares - they were all made with the longest strip back."]
["Several barrel spares for sector 3 were not made, because the corresponding double harnesses were used for tests"]
[]
["When using spares, it is the total length that is most important,"]
["as long as the splice point isn't in a REALLY bad place."]
["Sector 9","types","Number of spares","type 2","total length",null,"received","used"]
[]
["Sector 9 gap 29"]
[]
["barrel","longest",8,12.3,28.1,null,"NO"]
["EC","type 1",0,9.7,"N/A",null,"NO"]
[null,"type 2",2,9.7,23.8]
[null,"type 3",1,9.7,23.8]
[null,"type 4",2,9.7,23.8]
[null,"type 5",3,9.7,23.8]
[null,"type 6",2,9.7,23.8]
[null,"type 7",0,9.7,"N/A"]
[null,"type 8",3,9.7,23.8]
[null,null,13]
[]
["Sector 9 gap 35"]
[]
["barrel","2+2+2",6,11.5,29.7,null,"NO"]
[]
["Sector 9 gap 35 to level 2"]
[]
["EC","type 3",2,8.9,26.5]
[null,"type 5",2,8.9,26.5]
[null,"type 7",1,8.9,26.5]
[null,"type 8",1,8.9,26.5]
[null,null,6]
["Sector 9 gap 35 to level 5"]
[]
["EC with 10.3m type 2","type 3",1,10.3,27.2]
[null,4,2,10.3,27.2]
[null,5,2,10.3,27.2]
[null,8,1,10.3,27.2]
[null,null,6]
["EC with 11.3m type 2","type 5",1,11.3,27.2]
[null,7,1,11.3,27.2]
[null,8,1,11.3,27.2]
[null,null,3]
[]
["Sector 3","types","Number of spares","type 2","total length"]
[]
["barrel","mixture","<6",9,27.2,null,"4 T3",1,"used for 2031906"]
[null,"mixture","<8",10.3,28.7,null,"2 T2"]
[]
["EC - compact patch panel","type 9",1,7.7,27.4,null,"yes"]
[null,"type 12",1,7.7,27.4,null,"yes"]
[]
["EC - normal","type 5",1,7.7,27.4,null,"yes"]
[null,"type 6",1,7.7,27.4,null,"yes"]
[null,"type 7",1,7.7,27.4,null,"yes"]
[]
[]
[]
["Sector 1","types","Number of spares","type 2","total length"]
[]
["barrel ","mixture",12,8.6,30,null,"yes"]
[]
["end cap","type 1",2,5.9,25,null,"yes"]
[null,"type 2",2,5.9,25,null,"yes"]
[null,"type 3",2,5.9,25,null,"yes"]
[null,"type 4",4,5.9,25,null,"yes"]
[null,"type 5",4,5.9,25,null,"yes"]
[null,"type 6",2,5.9,25,null,"yes"]
[null,"type 7",4,5.9,25,null,"yes"]
[null,"type 8",2,5.9,25,null,"yes"]
[]
[]
[]
["Sector 7","types","Number of spares","type 2","total length"]
[]
["barrel ","mixture",6,10.4,30.2]
[null,"none",0,9,"N/A"]
[]
["endcap","type 1",0,7.7,"N/A"]
[null,"type 2",2,7.7,28]
[null,"type 3",1,7.7,28]
[null,"type 4",2,7.7,28]
[null,"type 5",3,7.7,28]
[null,"type 6",2,7.7,28]
[null,"type 7",0,7.7,"N/A"]
[null,"type 8",3,7.7,28]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}