DC/DC Converter 25/30 Watt TEN 25 Series

pdf-datasheet (52KB) pdf-Datenblatt (52KB)

Wide 2:1 Input Range Very high Efficiency Continuous Short Circuit Protection Overvoltage Protection Input Filter to meet EN 55022, Class A and FCC, Level A Remote on/off Adjustable Output Voltage Six-side shielded Metal Case with insulated Baseplate Industry Standard-Pinout

Line regulation: ±0.3% max. Load regulation: - Single output models: ±0.5% max. - Dual output models: ±1.0% max.

Output voltage adjustment: ±10% (by external resistor) Ripple & noise: <80 mVpk-pk (20 MHz BW) Conducted EMI: EN 55022, class A and FCC, level A (internal filter) Short circuit protection: continuous Efficiency: 85% typ. Operating temperature range: -40°C ... +71°C above 50°C derating 1.25%/°C I/O isolation voltage: 1’500 VDC Safety standards/ approvals: cUL/UL 1950, IEC/EN 60950 MTBF: >1 Mio. h @ +25°C Case: metal, 6-side shielded with insulated baseplate Remote on/off: shutdown input (remote on/off) for low input current (5 mA) in standby operation

Standard Models

Order code      Input voltage    Output         Output

                                voltage   current max.

TEN 25-1210                     3.3 VDC        5500 mA
TEN 25-1211                       5 VDC        5000 mA
TEN 25-1212      9 - 18 VDC      12 VDC        2500 mA
TEN 25-1213                      15 VDC        2000 mA
TEN 25-1222                    ± 12 VDC      ± 1250 mA
TEN 25-1223                    ± 15 VDC      ± 1000 mA

TEN 25-2410                     3.3 VDC        5500 mA
TEN 25-2411                       5 VDC        5000 mA
TEN 25-2412     18 - 36 VDC      12 VDC        2500 mA
TEN 25-2413                      15 VDC        2000 mA
TEN 25-2422                    ± 12 VDC      ± 1250 mA
TEN 25-2423                    ± 15 VDC      ± 1000 mA

TEN 25-4810                     3.3 VDC        5500 mA
TEN 25-4811                       5 VDC        5000 mA
TEN 25-4812     36 - 75 VDC      12 VDC        2500 mA
TEN 25-4813                      15 VDC        2000 mA
TEN 25-4822                    ± 12 VDC      ± 1250 mA
TEN 25-4823                    ± 15 VDC      ± 1000 mA

Pin-Out

Pin

 1
 2
 3
 4
 5
 6
 7
 8

   Single output

     +Vin(Vcc)
     -Vin(GND)
      No pin
   Remote on/off
      No pin
       +Vout
       -Vout
       Trim

                  Dual output

                   +Vin(Vcc)
                   -Vin(GND)
                    No pin
                 Remote on/off
                     +Vout
                    Common
                     -Vout
                     Trim

last Update: 12/02