DC/DC Converter 40 Watt TSI-40N Series

pdf-datasheet (215KB)

Step-down Switching Regulator Synchronous Rectification for ultra high Efficiency No Heat Sink required Adjustable Output Voltage Remote ON/OFF Continuous Short Circuit Protection Low Output Noise Small DIL-Package

Line regulation: ±0.5% max. Load regulation: ±0.5% max. Output voltage rangre: adjustable by ext. resistor Transient response time: 240 μsec. (50-100% load step) Ripple & noise: < 50 mVpk-pk typ. (20 MHz BW) Short circuit protection: continuous Efficiency: 94% typ. Operating temperature range: -10°C ... +71°C (with forced air cooling) MTBF: >900’000 h @ +25°C Remote on/off: shutdown input for low current (4.5 mA typ. for TSI40-1210/ 100 μA for TSI40-1211) in standby operation

Standard Models

 Order code      Input voltage      Output voltage     Output
                                 (adjustable range)   current max.

 TSI 40-1210     4.5 - 13.6 VDC        3.3 VDC           12 A
                                   (1.0...3.3 VDC)

 TSI 40-1211     8.0 - 13.6 VDC         5.0 VDC           8 A
                                   (5.0...6.0 VDC)

Pin-Out

Pin

  1

       Remote on/off

  2
  3
  4
  5
  6
  7
  8
  9
 10
11/12

        Signal GND
        +Vin(Vcc)
      -Vin(GND)/-Vout
       No function
        -Sense
      -Vin(GND)/-Vout
        +Vout
        +Sense
       No function
        Vout adj.

last Update: 05/02