MP/TJF UCL 24 JUL 00

8

8 x SEQUENCER OUTPUT

READ / WRITE ACCESS FROM VME

ENSA Reg.

VME ADDRESS BUS

15 BIT COUNTER

15 15

15

16 16

1

16

CLK ROD BUSY OUT Reg.

VME ROD CRATE BUSY OUT

ROD BUSY 7 - 21 16 x BUSY INPUTS FROM P3

16

16

16 2

10 10

12 12

24 24

CLK4A IDFER

SAL1ID

24 - bit COUNTER

SABCID

12 - bit COUNTER

TTYPE

10 - bit Reg.

ROD BUSY MASK Reg.

ENSEQ Reg.

SAECR2

SABCR2

L1ID

BCID

TTYPE

24 12 10

IDTRIG IDECR

READ / WRITE ACCESS FROM VME

TIM - SCH - 04

SEQTRIG

SEQBCR

SEQECR

SEQCAL

SEQFER

SEQSPARE

SEQTT

SEQID

ATLAS - SCT "TIM" SCHEMATICS 3 : ID & SEQUENCER / SINK

0 1 2 3 4 5 6 7

8 x 32 K RAM OE WREN

ADDRESS

8

0 - 7 SINK 8 x 32K RAM VME READ 8 8

ENSINK Reg.

TTIDIN 10

1

BCNTIN Reg. 12 1 BCNTIN Strobe

Strobes 2 SEQUENCER

SINK DATA

Strobe

Reg. Reg.