ZEUS MVD C & C MASTER REGISTERS -2-

MASTER VME

FINE TEST PULSE & CALIB. TRIGGER DELAY

VME address

BASE ADDRESS + 10

MASTER VME

FINE HCLOCK DELAY

VME address

BASE ADDRESS + 12

MASTER VME

VME address

BASE ADDRESS + 14

COARSE 0(LSB) (in steps of 1 CLK) 1 2 3 4 5 (MSB)

FINE 0 (LSB) (in steps of 0.5ns) 1 2 3 4 5 6 7 (MSB)

1 2 3 4 5 6 7 (MSB)

(in steps of 0.5ns)

FINE 0 (LSB)

MP/TJF, HEP - UCL 18/02/2000

PROGRAMMABLE DELAYS

COARSE CALIB. TRIGGER DELAY

TEST PULSE 0 (LSB)

(in steps of 1 CLK)

COARSE TEST PULSE DELAY

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15(MSB)