ZEUS MVD C & C SLAVE REGISTERS

SLAVE VME

GFLT CONTROL VME address

BASE ADDRESS + 02

SLAVE

COARSE 0(LSB) (in steps of 1 CLK) 1 2 3 4 5(MSB)

FINE 0 (LSB) (in steps of 0,5ns)

VME

GFLT NUMBER VME address

BASE ADDRESS + 00

VME

VME address

BASE ADDRESS + 04

ADCs

BUSY F/ERROR

ERROR (R/R)

ROSYS 0 1 ROAMB 0 1 ROUSR 0 1 2 A/ABORT A/ACCEPT

FLTN

GBCN

1 2 3 4 5 6 7

0

1 2 3 4 5 6 7

0

MP/TJF, HEP - UCL 18/02/2000

VME

VME address

BASE ADDRESS + 06

SLAVE

VSOA RESET

VF/ERROR

CLRTESTBUSY

SLAVE COMMAND

ADCs STATE

SLAVE VME

SLAVE STATE VME address

BASE ADDRESS + 08

A/CLK ON

A/RESET

TESTBUSY

VBUSY

VERROR(R/R)

ENTESTBUSY

B/PLANE EMPTY B/PLANE BUSY B/PLANE F/ERR B/PLANE ERROR B/PLANE RESET B/PLANE ABORT B/PLANE ACCEPT

B/PLANE STATE

LASTTRIGABORT