{"text_format":"5","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"props":{"creator":"warren","last_modified_by":"Matthew Warren","company":"UCL"},"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":39,"n_cols":10,"rows_kept":39,"flags":["formulas_cached_only"]}
["HD PSU Wiring"]
["Signal","D15 VME conn.","PSU->VME cable","Inside PSU","SSR","IDC ribbon col","10 way AWG ribbon","5 way SIL socket","3 way AWG SSR (grn)","3 way AWG Serial (blu)"]
["VME/DC"]
["+3.8V","1, 2, 9","yel, turq, wht","yel",null,"4 yel"]
["-1.2V","4, 11, 12","pink, blk, brn","pink",null,"1 brn"]
["-5V",6,"grey","grey",null,"8 grey"]
["+3.8Vs",10,"ora","ora",null,"3 ora"]
["-1.2Vs",3,"red","red",null,"2 red"]
["-5Vs",14,"viol","viol",null,"7 viol"]
["VME+5",13,"blue","blue","blu/wht","6 blu"]
["VME0V","5, 7","grn","grn/yel",null,"5 grn"]
["Remote Overide",{"$nulls":3},"pnk/wht","9 wht"]
["[IDC spare]",{"$nulls":4},"10 blk"]
["Controller"]
["Stat LED a",{"$nulls":5},"1 brn"]
["Stat LED k",{"$nulls":5},"2 red"]
["[10 way AWG spare]",{"$nulls":5},"3 ora"]
["[10 way AWG spare]",{"$nulls":5},"4 yel"]
["Reset 1",{"$nulls":5},"5 grn"]
["Reset 2",{"$nulls":5},"6 blu"]
["[10 way AWG spares]",{"$nulls":5},"7-10"]
["Temp. Sensors"]
["+2.56V",{"$nulls":6},"3 red"]
["-2.56V",{"$nulls":6},"4 blk"]
["Temp1 (module 1)",{"$nulls":6},"2 yel"]
["Temp2 (module 2)",{"$nulls":6},"1 viol"]
["key (n/c)",{"$nulls":6},"5"]
["SSR"]
["Controller SSR",{"$nulls":7},"1 wht"]
["VME+5",{"$nulls":7},"2 yel"]
["[key",{"$nulls":7},"[key]"]
["Serial"]
["0V",{"$nulls":8},"1 grn"]
["TX",{"$nulls":8},"2 wht"]
["RX",{"$nulls":8},"3 pink"]
[]
[]
[]
["*Note: the VME+5 interlock is replaced by the 3.8V from this PSU in the FP D15 conn"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}