{"text_format":"5","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"props":{"creator":"HEP","last_modified_by":"HEP","company":"UCL"},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":30,"n_cols":16,"rows_kept":30,"flags":["formulas_cached_only"]}
["PB PSU Wiring"]
[null,"Panel to ext conns","7 way AWG on LED Panel","Test Point","Test point position","9 way AWG on LED Panel","2x 5 way SIP","Test Point wires"]
["LED Panel"]
["-5s","brn",1,"brn","1 top",1]
["+5s","pnk",2,"pnk",2,2]
["+2.1s cont","red",3,"red",3,3]
["-1.2s cont","blu",4,"blu",4,4]
["+2.1s clk","ora",5,"ora",5,5]
["-1.2s clk","yel",6,"yel",6,6]
["0V","blk",7,"blk","7 lower",7]
["[key]",{"$nulls":4},"[key]"]
["[spare]",{"$nulls":4},"[spare]"]
["LED Panel (VME)"]
["+3.8s",null,null,"wht",8,null,1]
["-1.2s",null,null,"vio",9,null,2]
["-5s",null,null,"gry",10,null,3]
["VME 0V",null,null,"grn","11 bot",null,5]
["[key]",null,null,"[key]",null,null,4]
["Serial"]
["0V",{"$nulls":11},792,1200,2200,776.4705882352941]
["RX"]
["TX"]
["Controller Panel"]
["[spare] (stat_led_a)"]
["[spare] (stat_led_k)"]
["Reset 1"]
["Reset 2"]
["Override"]
[]
["[10 way AWG spares]"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}