5 5

MASTER STATE

VME address

7 7

MASTER COMMAND

VME address

NOTE:

MP/TJF, HEP - UCL 27 JULY 98

+

+

ZEUS MVD C & C MASTER WIRE-WRAP PROTOTYPE

Base Address + 02

MASTER VME

Base Address + 00

MASTER VME

V_TRIGGER //

+

+ V_ERROR + V_BUSY + VOT_RESET + V_CALIBRATE

+

+ // + V_O/ALL_RST

+

+

ACCEPT ERROR BUSY_OUT OT_RESET CALIBRATE_BUSY

these commands will generate a SINGLE command by writing "1" to the appropriate bit, and must be returned to "0" following each single command

see description in par. m) and p)

these commands are asserted by writing "1" to the appropriate bit, and will remain asserted until "0" is written to that bit

ENVAR_TRIG