GG magnet diameter is approx. 188.5 where iron triangles are situated.

GG is centred in the RCAL gap which is 200 across and 236 high

200

236

Section through RCAL and GG at Z = approx. -2920 29.11.00

Cables enclosed in ’zippertube’ Cables are held flat and bundles restrained around GG with no cables at the sides.

Combo cables - 5 in each barel set, 4 in each wheel set, 44 bundles in total.

Radiation monitor cables (round, red) Alignment cables (flat, orange) Thermal sensors (round, black) cable restraint