Al / Kapton 100μm (Al 50μ, glue 25, Kapton 25) glue 25μm

275μ

’Model’ Low Mass Cable

(made up at UCL)

what effect does cooling at -7 C have on this? no change after several days testing

Kapton 25μm

2 layers of glue 25 thick - 50 2 layers of Al coated Kapton 100 thick - 200 1 outer Kapton coverlay 25 thick - 25

Kapton coverlay

glue Al / Kapton

Al / Kapton glue

NB : the Aluminium layer is continuous, ie is not composed of ’tracks’