One Harness* showing 6 sections (extends across half the Barrel) seen from the side facing the barrel surface, with optoboards and fibres (2 going to red ribbon and 1 going to blue ribbon from each board.

*System test 98 design

TJF 2.9.98

6 double power tapes at end of barrel go off to patch panel outside perimeter of largest barrel tracks on dog leg connect to tracks on long power tapes (possibly soldered)