123.5

249.4

371.3

498.0

618.3

43.0 31.3

107.4

43.0 TYP

754.3

40.0

84.0

35.0

34.0

OPTOPACKAGE REGION

STRAPS HELD USING CAPTIVE SCREWS

CLEAR PERSPEX COVER FORMED TO HARNESS SHAPE

BEND

BEND

OPEN SLOTS LOCATE ON MODULE FIXATION POINTS ON BRACKET (large clearance)

20mm radius

POSITION OF ALL STRAPS CLEAR OF CONNECTORS OPTO FIBRES AND OPTO PACKAGE

HARNESS

LARGER STRAP RETAINING END BARREL TAPES

HARNESS COVER - VERSION 2 (allows for harness installation before cooling installation) TJF UCL 24.11.00

HARNESS COVER VERSION 2

(allows for harness installation before installation of cooling) TJF 24.11.00