HORIZONTAL INTERLINK

HORIZONTAL INTERLINK

6 5

4 3

6 4

6 5 5 5 5 4 4

6 6 6

4 3 3 3

6 5

SHORT INTERLINK

ATLAS SCT BARREL END SERVICES - barrels 3, 4, 5 and 6 out to thermal enclosure

evap. Cooling exhaust pipes input capillary tubes - routed separately from exhaust tubes over or under tapes. alignment light path tubes evap. cooling exhaust manifold distribution manifold

optical fibre ducting low mass power tapes (6 in each set) tape sets from barrels as shown

VERSION 2 26 05 2000