R 284

R 285.4

R 288

R 291

R 299

M3clear - position according to position of cooling exhaust manifold

M2 tapped

20 10

11.25

11.25

22 22 1.0 8.0

M2 5 deep full thread

5

prototype machined from 8mm thick PEEK. Mass of structure to be minimised by removal of excess material. 110 fibre splice bunch

5

DRW016 A-F

HARNESS END CLAMP MULTISTRUCTURE FOR ATLAS SCT BARREL COOLING MANIFOLD AND READOUT OPTICAL FIBRE SUPPORTAND POWER TAPE CLAMP.