optofibre loops round this side of dogleg from behind and over clamp or round it if more length is required.

gap here allows optofibre to pass through when installing clamp and join ribbon in this space

optoribbon 12 way and 8 way held by clamp near lower edge of low mass tape to allow for bigger loop.

r = 20mm

New type of on-barrel cable clamp - a modified version of the original Geneva clamp

TJF 12.7.99

Clamp is lengthened here for system test in order to clear connectors joining dogleg and tape, but may not be necessary if solder join is used barrel end