ATLAS - SCT Model Barrel Harnesses

STATUS at 12th June 1998^{TJF}_{12.6.98}

2 model harnesses have been made using the following procedure:

1) Laminated strips were made up (see other page) and cut to size: 1.8 meters long x 18mm wide with 2 layers of Al/Kapton separated at one end.

2) Dog Legs made from one layer of Al/Kapton and one layer of Kapton + glue layer

3) Mock connectors and mock optoboards attached to Dog Legs

4) Tapes and Dog Legs connected on bench using a template to position each set

* Tapes restrained with Velcro hinged cable clamps between each set and at cable ends during each stage of assembly

5) Mock optofibre ribbon strip laid and optofibres glued to optoboards

6) With cable clamps securing tapes, Dog legs and opto ribbon, the harness is taken to the barrel and mounted, the cable retainers replacing cable clamps as each module set is mounted