R 284

R 285.4

R 288

R 290

R 299 20 10

11.25

11.25

22 22 1.0 8.0

M2 5 deep full thread for connection to castellation

5

110 fibre bunch 54 fibers max in 0.9mm OD single tubing (6.3 x 8.1mm)

5 slot for cooling manifold attachment - lateral position varies with manifold position

Clip to secure fibre bunch max 54 fibres <M1.6 tapped holes for clips at intervals along structure

New version- Structure for harness end clamp/ fibre routing from harness to duct/ cooling exhaust manifold support. TJF 5/7/01

all excess material removed

M2 tapped tapped holes for fibre clip - use only where necessary

moulded/machined from PEEK or Vectra A130