Windows for Optopackage components

thinner section profile to match bracket ’bar’. Protects emerging fibres

optofibres covered with Kevlar sleeve which extends from under optopackage cover out to junction with optoribbon

Bracket bar cover clears all components by 0.5 to 1mm

cover glued to dogleg in area surrounding optopackage

15mm 2mm?

5mm

30mm

Drawing of Optopackage cover as shown on photo All surfaces rounded - no sharp edges

dogleg

Dimensions depend on dimensions of optopackage

smooth molded plastic cover

TJF - UCL 14/10/99