12 fibres sleeved in furcation tubing

’Sumitube’ heatshrink tubing furcation tubing staggered termination with ’bare’ fibre to splice fibre splice protector covered by heatshrink

12 way fibre ribbon

40mm long x 5.5 wide x 2.25 thick rigid

60mm long x 4.5 wide x 1.8 thick flexible in one plane bunch diameter 4.8mm reducing to 3.7 x 3.1 100mm long - not very flexible

12 fibres each 0.9mm diam. flexible

total length of heatshrink tubing 205mm

3.2mm wide x 0.3 thick flexible in one plane

Dimensions of sample section of spliced optical readout fibre from Taiwan June 2002 (for barrel harness)

TJF 27.06.2002 note: bend radius of fibre limit 20mm note: black tube may have larger diameter