765 770 775 780 785 790 795 800

Z

792

783.5

R531

R550

R540

R554

R520

R510

R500 R498

LIGHT PATH TUBE

THERMAL ENCLOSURE

LOW MASS TAPES - one harness - another barrel

LOW MASS TAPES - one harness - one barrel

ALIGN. SOCKET

ALIGNMENT T POST

BARREL FLANGE REGION

TRT SERVICES ENVELOPE

tooling ring ins.

1.5

6.5

7.5

3mm approx. with shielding wrap ?

?

on-barrel manifold on-barrel manifold

SCT COOLING PIPES

COOLING MANIFOLD WITH BELLOWS

SCT COOLING PIPES

11

6

THERMAL ENCLOSURE

?

?

MOVE PIPE BY 3.5 AWAY FROM TAPES ie TO MID-WAY BETWEEN 775 and 792 extend

3

3

2.5

5.5