ATLAS SCT BARREL modelling and prototyping work at UCL

ON-BARREL items:

clearances at barrel end, trials with latest dimensions for LM tapes, barrel end clamps, fibres, PCB, interlink cable, and dogleg.

ONGOING -

need ’final’ thickness of LMTs

need to check castellation, straps and bracket pad hooks when Barrel 3 is at Geneva

need to check manufactured interlink cables 4 types

revisit removal of last redundancy arm dogleg 6

trials with latest design of harness clip related to clearances of dogleg and module, movement in phi of dogleg; use on Geneva dogleg jigs.

barrel end harness clamp - trials with modified design when final thickness of LMTs is known, properties of castellations and straps are known.

Barrel end up to and including PPB1:

ONGOING-

Harness lengths check: need final dimensions of readout fibre splice protector in order to finalise/revise fibre lengths and finalise end barrel fibre ducting dimensions also need to know type of light-proof covering to be used on sections of ribbonised fibre - new dimensions/flexibility.

updates from the Valencia meetings TJF 18.06.2002

will be maximum of 0.350mm but wait for production sample

not possible

see diagram of splice protector 27.6.02 trials on Prototype Sector at RAL

trials on Prototype Sector at RAL