KITTING LIST for: PC3116M OM Job No:

April 18, 1999 Page 1 of 1

Engineer Designer PC Issue Circuit Issue Qty Cost Centre

Checked & Approved (Signed & dated) M.POSTRANECKY D.J.BECKETT 2 B

Comp Ref Manufacturer & Part No or Supplier's Name & Part No

Part Description

Board Qty Kit Qty Kit Kit Kit Kit Not Issued

Check Comments

C1 FARNELL 920-447 220UF 16V ELECTROLYTIC 1 -
C2-14 FARNELL 262-547 100NF 100V CERAMIC CAPACITOR 13 -
DS1 SCHROFF 69004-122 STANDARD GREEN 3.2MM LED 1 -
FS1 FARNELL 514-962 10A WIRE ENDED FUSE 1 -
J1 J2 RAL STORES 61/00820 96WAY RT-ANG VERO PLUG 905-72178F 2 -
J10-17 3M 3793-5302 10WAY RT-ANG IDC HEADER, CLASS II 8 -
JAUX ERNI(STUC3) 30-M-ABC 30WAY RT-ANG PCB PLUG 1 -
PL1-7 HARWIN M20-999 02 05 HARWIN STRAIGHT 2 PIN HEADER 7 -
R1-6 FARNELL 543-305 470R RESISTOR, 0.25W 6 -
RN1 RN7 FARNELL 107-055 100R, 4-ISOLATED RESISTORS, 200MW 2 -
RN2-6 FARNELL 148-980 470R, 8-COMMONED RESISTORS, 200MW 5 -
SW1 OMRON A6D4100 4WAY DIL SWITCH 1 -
U1 U2 MOTOROLA MC10115P QUAD DIFFERENTIAL LINE RECEIVER 2 -
U3-6 MOTOROLA MC10101P QUAD OR/NOR GATE 4 -
U7 MOTOROLA MC10105P TRIPLE 2-3-2-INPUT OR/NOR GATES 1 -
- PC3116M/2 PC BOARD 1
- VERO 957-244797B VERO KM6 6Ux4HP TYPE C FRONT PANEL KIT 1
- VERO 173-44767C FRONT PANEL MOUNTING BRACKETS 2
- HARWIN D2816-01 16-PIN LOW PROFILE IC SOCKETS 7 AVAILABLE FROM FARNELL 741-103
- HARWIN DO1-9972001 SIL SOCKET STRIPS 4 4x20-WAY STRIPS REQUIRED
- HARWIN M7567-05 2-WAY JUMPER SOCKET 7
- ELECTROSPEED 19-38208F WIRE-ENDED FUSE HEADERS 2 2 HEADERS REQUIRED FROM STRIP OF 20