PIN Array Specifications

The 12 way PIN arrays should have common cathodes and individual anodes. Technical specifications are shown in table 1 below.

Characteristics Min. Typical Max. Units Operating wavelength 820 840 860 nm Input power 3 mW Responsivity @ 820 -860 nm 0.4 0.5 A/W Dark current <1 2 nA Reverse voltage 1 10 V Breakdown voltage 15 V Rise/Fall time <1 2 ns Device reliability 350 FIT

Table 1: Technical specifications for the PIN-diode arrays