ORDERING LIST for: initial OM Job No:

October 4, 1999 Page 1 of 2

Engineer Designer PC Issue Circuit Issue Qty Cost Centre

Checked & Approved (Signed & dated)

M.POSTRANECKY D.J.BALLARD 1 A

Comp Ref Manufacturer & Part No or Supplier's Name & Part No

Part Description

Board Qty Total Qty Qty Ordered

Purchase Order No

Order Date

Supplier

Goods In Comments

C1 AVX-KYOCERA TAJD226K016R 22UF SMD 16V CAPACITOR, CASE SIZE D 1 AVAILABLE FROM FARNELL 498-749

C2-45 C50 C52 C54-
98 C100 C102-105
C108

                     RS 264-4416 100NF SMD CAPACITOR, 0805, X7R DIELEC-
                                                   TRIC, 50V

                                                                                              97 -

C46-49 C51 C53 C106
C107

                     RAL STORES 59/24923 10NF, HI-K CERAMIC REDCAPS OR BLUE MAX
                                                   CAPACITOR

                                                                                              8 -

C99 FARNELL 912-967 1000UF 16V AXIAL ELECTROLYTIC 1 -

C101 FARNELL 920-460 470UF 16V ELECTROLYTIC 1 -

DL1 DDD PDU-15F-1 PROGRAMMABLE DELAY UNIT, TTL 1NS STEPS 1 -

FS1 FARNELL 514-962 10A WIRE ENDED FUSE 1 -

FS2 FARNELL 319-326 5A WIRE ENDED FUSE 1 -

J1 J2 RAL STORES 61/00820 96WAY RT-ANG VERO PLUG 905-72178F 2 -

JAUX ERNI(STUC3) 30-M-ABC 30WAY RT-ANG PCB PLUG 1 -

PL1-4 3M 3431-D303 34-PIN CONDO DOUBLE-HEADER, PCB RT-ANG 4 -

PL5 PL10 HARWIN M20-999 03 05 HARWIN STRAIGHT 3 PIN HEADER 2 CAN BE CUT FROM M20-999 36 05

PL6 PL15-21 HARWIN M20-999 02 05 HARWIN STRAIGHT 2 PIN HEADER 8 CAN BE CUT FROM M20-999 36 05

PL8 PL9 3M 3432-6002 40WAY STRAIGHT IDC CONNECTOR WITH NO
                                                   EJECTOR/LATCH

                                                                                              2 -

PL101 3M 3431-5302 34WAY RT-ANGLE IDC HEADER 1 -

R1 FARNELL 543-627 10K RESISTOR, 0.25W 1 -

R2 FARNELL 543-482 2K7 RESISTOR, 0.25W 1 -

R3 R4 FARNELL 543-380 1K0 RESISTOR, 0.25W 2 -

R5-15 FARNELL 911-859 1K0 SMD RESISTOR, 0.1W, 0805 11 -

R16-65 FARNELL 911-940 5.6K SMD RESISTOR, 0.1W, 0805 50 -

RN1 RN2 FARNELL 148-983 4K7, 8-COMMONED RESISTORS, 200MW 2 -

RN3 RN16 RN17 RN22
RN23 RN26 RN27 RN30
RN31 RN34 RN35

                     OM STORES 120R 120R, 4-ISOLATED RESISTORS, 200MW 11 -

RN4 RN5 RN9 RN10
RN19 RN21 RN24 RN25
RN28 RN29 RN32 RN33
RN36 RN37

                     ARROW 095474D 390R, 8-COMMONED RESISTORS, 200MW 14 MOQ = 5000

RN18 FARNELL 148-981 1K, 8-COMMONED RESISTORS, 200MW 1 -

SW1 SW2 ERG SDS8014 8WAY DIL SWITCH 2 AVAILABLE FROM FARNELL 422-666

U1 U9 U10 U18 U19
U26 U27 U32 U33 U40
U41

                     MOTOROLA MC10125P QUAD ECL TO TTL TRANSLATOR 11 -

ORDERING LIST for: initial OM Job No:

October 4, 1999 Page 2 of 2

U2 LATTICE GAL22V10B-15LP EE CMOS PLD 1 -

U3 U24 U25 U37-39
U45 U49 U50

                     AMD MACH210-10JC EE CMOS PLD, 38I/P 32O/P 9 PTH SOCKET REQUIRED FOR THIS DEVICE

U4-7 U12 U14 U20
U21 U28 U29 U34 U35
U42 U43

                     MOTOROLA MC10124P QUAD TTL TO ECL TRANSLATOR 14 -

U8 U13 TI SN74LS05N HEX INVERTORS WITH OPEN-COLLECTOR OUTPUTS 2 -

U11 MOTOROLA MC10192P QUAD BUS DRIVER 1 -

U15 U22 U30 U36 U44 NSC 74F541PC OCTAL BUFFERS, 3-STATE OUTPUTS 5 -

U16 TI SN74F244N 3-STATE OCTAL BUFFER 1 -

U17 TI SN74LS14N HEX SCHMITT-TRIGGER INVERTERS 1 -

U23 TI SN74F240N OCTAL BUFFERS AND LINE DRIVERS WITH 3-
                                                   STATE OUTPUTS

                                                                                              1 -

U31 AMD MACH230-15JC EE CMOS PLD, 70I/P 64O/P 1 PTH SOCKET REQUIRED FOR THIS DEVICE

U46-48 AMD AM29F010-90JC 128K X 8-BIT SECTOR ERASE FLASH MEMORY 3 PTH SOCKET REQUIRED FOR THIS DEVICE

U51 EUROQUARTZ LK41670C 40.670MHZ CRYSTAL CLOCK OSCILLATOR 1 -

Comp Ref Manufacturer & Part No or Supplier's Name & Part No

Part Description

Board Qty Total Qty Qty Ordered

Purchase Order No

Order Date

Supplier

Goods In Comments