ORDERING LIST for: PC3183M OM Job No:

February 8, 2001 Page 1 of 2

Engineer Designer PC Issue Circuit Issue Qty Cost Centre

Checked & Approved (Signed & dated)

M.POSTRANECKY D.J.BECKETT 2 B

Comp Ref Manufacturer & Part No or Supplier's Name & Part No

Part Description

Board Qty Total Qty Qty Ordered

Purchase Order No

Order Date

Supplier

Goods In Comments

- PC3183M/2 PC BOARD 1 -

- ELECTROSPEED 953-236016G KM6-II TYPE C FRONT PANEL 6Ux4HP 1 SEE DRAWING A2-TE-0103-016-01-* FOR HOLE DETAILS

- ELECTROSPEED 173-44767C METAL FIXING BRACKETS (PK OF 10) 1 2 BRACKETS REQUIRED PER BOARD

C1-49 C52 C55 C58
C61 C64 C67 C70
C73-102 C107-116
C119 C122 C125 C128
C131 C134 C137 C140
C143-163 C167-225
C227-232 C234 C235

                     AVX-KYOCERA
                     CM21X7R104K25VAT

                                                   100nF SMD Capacitor, 0805 192 Available from FARNELL 499-687

C50 C53 C56 C59 C62
C65 C68 C71 C121
C124 C127 C130 C133
C136 C139 C142 C164

                     AVX-KYOCERA 08055C103KAT00J 10nF SMD Capacitor, 0805 17 Available from FARNELL 499-225

C51 C54 C57 C60 C63
C66 C69 C72 C120
C123 C126 C129 C132
C135 C138 C141 C165

                     AVX-KYOCERA 08055C102KAT00J 1nF SMD Capacitor, 0805 17 Available from FARNELL 499-201

C103 C233 Farnell 920-460 470uF 16V Electrolytic 2 -

C104-106 RS 394-557 1000uF 6.3V Radial Electrolytic, Low ESR 3 -

C117 C118 AVX-KYOCERA TAJB475K016R 4.7uF SMD 16V Capacitor, Case Size B 2 Available from FARNELL 498-725

C166 Philips 037 56479 47UF General Purpose Capacitor, 037
                                                   Series

                                                                                              1 Available from Farnell 286-369

C226 Farnell 303-665 1000pF, 100V Med-K Capacitor, 630 Series 1 -

D1-47 RS 266-2329 Voltage Reference Diode 47 -

DS1 RS 309-5304 Tri-Level Red/Yellow/Green 3.0mm LED 1 -

DS2 HP HSMS-C670 Surface Mount Flip-Chip Red LED, with
                                                   80mm Flexible Light Pipe

                                                                                              1 LED avail. from Farnell 491-949, also order
Flexible Light Pipe Farnell 324-5305

DS3 HP HSMY-C670 Surface Mount Flip-Chip Red LED, with
                                                   80mm Flexible LIght Pipe

                                                                                              1 LED avail.from Farnell 549-514, also order Flex-
ible Light Pipe Farnell 324-5305

DS4 HP HSMG-C670 Surface Mount Flip-Chip Red LED, with
                                                   80mm Flexible LIght Pipe

                                                                                              1 LED avail.from Farnell 491-962, also order Flex-
ible Light Pipe Farnell 324-5305

FS1 Farnell 319-326 5A Wire Ended Fuse 1 -

FS2-4 Farnell 319-302 2A Wire Ended Fuse 3 -

J1 J2 RAL Stores 61/00820 96way Rt-Ang Vero Plug 905-72178F 2 -

LK1-5 Comatel 3000500 2 pin 0.6 inch pitch Jumper 5 -

PL1 PL2 3M 3431-D303 68-Pin Condo double-header, PCB RT-ANG 2 -

PL3 3M 3428-D303 40-Pin Condo double-header, PCB RT-ANG 1 -

PL4 3M 3910-0000T 10-Pin IDC PCB DIP Connector 1 -

ORDERING LIST for: PC3183M OM Job No:

February 8, 2001 Page 2 of 2

PL5 3M 3793-5602 10way Rt-Ang IDC Header, Class II 1 Available from Farnell 439-915
PL6-10 Harwin M20-999 20 05 Harwin Straight 1 pin Header 5 Can be cut from M20-999 20 05
PL11 Molex 22-03-2061 Molex Straight 6 pin Header, 0.1in pitch 1 Available from RS 479-181
PL12-17 Harwin M20-999 04 05 Harwin Straight 4 pin Header 6 Can be cut from M20-999 36 05
R1 R2 R59 Farnell 613-095 1K0 SMD Resistor, 0.1W, 0805 3 -
R3-6 Farnell 612-972 100R SMD Resistor, 0.1W, 0805 4 -
R7 R8 Farnell 613-290 47K SMD Resistor, 0.1W, 0805 2 -
R9 Farnell 612-959 68R SMD Resistor, 0.1W, 0805 1 -
R10-56 Farnell 613-198 6.8K SMD Resistor, 0.1W, 0805 47 -
R57 R58 R60-74 Farnell 613-216 10K SMD Resistor, 0.1W, 0805 17 -
RN1-7 Farnell 776-749 4K7, ARC241, 4-isolated Resistors, 0.062W 7 -
SW1-6 Farnell 146-199 Sealed PCB Mount Vert Rotary Hex Switch 6 Available from Farnell 146-199
U1 NSC DS90C032TM LVDS Quad CMOS Differential line Receiver 1 -
U2-20 NSC DS90C031TM LVDS Quad CMOS Differential line Driver 19 -
U21-28 U42-50 Dallas Semiconductor
                     DS1020S-50

                                                   Programmable 8-bit Silicon Delay Line 17 -

U29 Philips N74LS541N Octal Buffers with 3 State Outputs 1 -
U30 TI SN74LS123N Dual Monostable 1 -
U31 Lattice M5-256/120-15YC High Density PLD 1 -
U32 Lattice M5-192/120-7YC High Density PLD 1 -
U33 TI SN74F38N Quad 2 Input NAND Buffer 1 -
U34 Newport 50A10201 Active Buffered 10-Tap, 20ns Step Delay
                                                   Line

                                                                                              1 Available for Farnell 175-220

U35 U38 U41 NSC 74F543PC Octal Registered Transceiver 3 -
U36 U37 U39 U40 U51 Philips N74F541N Octal Buffers, 3-state outputs 5 -
- HARWIN D01 99010-01 HARWIN ULTRA LOW PROFILE SOCKETS REQUIRED FOR 4 20-PIN DIPS
- HARWIN D01 99012-01 HARWIN ULTRA LOW PROFILE SOCKETS REQUIRED FOR 4 20-PIN DIPS

- FARNELL 178-213 0.3” DECOUPLED IC SOCKET -

Comp Ref Manufacturer & Part No or Supplier's Name & Part No

Part Description

Board Qty Total Qty Qty Ordered

Purchase Order No

Order Date

Supplier

Goods In Comments