{"text_format":"5","workbook":"xls","n_sheets":1,"sheets":["PatchBox-to-Helix-Driver-Contro"],"props":{"creator":"mp","last_modified_by":"Matthew Warren","company":"UCL"},"not_rendered":{"external_links":1},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"PatchBox-to-Helix-Driver-Contro","index":0,"n_rows":139,"n_cols":15,"rows_kept":139,"flags":["formulas_cached_only"]}
[]
[]
["     CONTROL  SIGNALS  CABLE  CONNECTORS  AT",{"$nulls":8},"      CONTROL  SIGNALS  CABLE"]
["             PATCHBOX  CONTROL  DRIVER  PCBs",{"$nulls":8},"CONNECTORS AT HELIX DRIVER PCBs"]
[]
["PATCH-","PCB","B/PLANE","TEST-","NOT-","SERIAL","F/PANEL","CABLE","CABLE",null,"CABLE","OLD CABLE","CABLE","F/PANEL","PCB"]
["BOX","SLOT","CONNEC.","PULSE","RESET","LOAD","CONNEC.","MARKER","LABEL",null,"MARKER","LABEL","LABEL","CONNEC.","SLOT"]
[{"$nulls":6},"( 34-way )",{"$nulls":6},"( 34-way )"]
[]
["     A","slot 4","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","A-4-31",null,"BLUE","4-A-1","5-A-1","     A-1",4]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","A-4-32",null,"BLUE","4-A-2","4-B-1","     A-2"]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","A-4-33",null,"BLUE","4-B-1","4-A-2","     B-1"]
[]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","A-4-34",null,"BLUE","5-A-1","4-A-1","     A-1",5]
[]
[]
["     A","slot 10","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","A-10-31",null,"BLUE","5-A-2","6-A-2","     A-2"]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","A-10-32",null,"BLUE","5-B-1","6-A-1","     B-1"]
[]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","A-10-33",null,"BLUE","6-A-1","5-B-1","     A-1",6]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","A-10-34",null,"BLUE","6-A-2","5-A-2","     A-2"]
[]
[]
["     A","slot 16","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","A-16-31",null,"BLUE","6-B-1","7-B-1","     B-1"]
[]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","A-16-32",null,"BLUE","7-A-1","7-A-2","     A-1",7]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","A-16-33",null,"BLUE","7-A-2","7-A-1","     A-2"]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","A-16-34",null,"BLUE","7-B-1","6-B-1","     B-1"]
[]
[]
["     A","spare","  -","  -","  -","  -","( 34-way )","BLUE","A-spare",null,"BLUE","A-spare",null,"( 34-way )"]
[]
[]
[]
["     CONTROL  SIGNALS  CABLE  CONNECTORS  AT",{"$nulls":8},"      CONTROL  SIGNALS  CABLE"]
["             PATCHBOX  CONTROL  DRIVER  PCBs",{"$nulls":8},"CONNECTORS AT HELIX DRIVER PCBs"]
[]
["PATCH-","PCB","B/PLANE","TEST-","NOT-","SERIAL","F/PANEL","CABLE","CABLE",null,"CABLE","CABLE",null,"F/PANEL","PCB"]
["BOX","SLOT","CONNEC.","PULSE","RESET","LOAD","CONNEC.","MARKER","LABEL",null,"MARKER","LABEL",null,"CONNEC.","SLOT"]
[{"$nulls":6},"( 34-way )",{"$nulls":6},"( 34-way )"]
[]
["     B","slot 4","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","B-4-31",null,"BLUE","8-A-1","9-A-1","     A-1",8]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","B-4-32",null,"BLUE","8-A-2","8-B-1","     A-2"]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","B-4-33",null,"BLUE","8-B-1","8-A-2","     B-1"]
[]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","B-4-34",null,"BLUE","9-A-1","8-A-1","     A-1",9]
[]
[]
["     B","slot 10","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","B-10-31",null,"BLUE","9-A-2","10-A-2","     A-2"]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","B-10-32",null,"BLUE","9-B-1","10-A-1","     B-1"]
[]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","B-10-33",null,"BLUE","10-A-1","9-B-1","     A-1",10]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","B-10-34",null,"BLUE","10-A-2","9-A-2","     A-2"]
[]
[]
["     B","slot 16","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","B-16-31",null,"BLUE","10-B-1","11-B-1","     B-1"]
[]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","B-16-32",null,"BLUE","11-A-1","11-A-2","     A-2",11]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","B-16-33",null,"BLUE","11-A-2","11-A-1","     A-2"]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","B-16-34",null,"BLUE","11-B-1","10-B-1","     B-1"]
[]
[]
["     B","spare","  -","  -","  -","  -","( 34-way )","BLUE","B-spare",null,"BLUE","B-spare",null,"( 34-way )"]
[]
[]
[]
["     CONTROL  SIGNALS  CABLE  CONNECTORS  AT",{"$nulls":8},"      CONTROL  SIGNALS  CABLE"]
["             PATCHBOX  CONTROL  DRIVER  PCBs",{"$nulls":8},"CONNECTORS AT HELIX DRIVER PCBs"]
[]
["PATCH-","PCB","B/PLANE","TEST-","NOT-","SERIAL","F/PANEL","CABLE","CABLE",null,"CABLE","CABLE",null,"F/PANEL","PCB"]
["BOX","SLOT","CONNEC.","PULSE","RESET","LOAD","CONNEC.","MARKER","LABEL",null,"MARKER","LABEL",null,"CONNEC.","SLOT"]
[{"$nulls":6},"( 34-way )",{"$nulls":6},"( 34-way )"]
[]
["     C","slot 4","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","C-4-31",null,"BLUE","12-A-1",null,"     A-1",12]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","C-4-32",null,"BLUE","12-A-2",null,"     B-1"]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","C-4-33",null,"BLUE","12-B-1",null,"     B-1"]
[]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","C-4-34",null,"BLUE","13-A-1",null,"     A-1",13]
[]
[]
["     C","slot 10","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","C-10-31",null,"BLUE","13-A-2",null,"     A-2"]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","C-10-32",null,"BLUE","13-B-1",null,"     B-1"]
[]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","C-10-33",null,"BLUE","14-A-1",null,"     A-1",14]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","C-10-34",null,"BLUE","14-A-2",null,"     A-2"]
[]
[]
["     C","slot 16","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","C-16-31",null,"BLUE","14-B-1",null,"     B-1"]
[]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","C-16-32",null,"BLUE","15-A-1",null,"     A-1",15]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","C-16-33",null,"BLUE","15-A-2",null,"     A-2"]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","C-16-34",null,"BLUE","15-B-1",null,"     B-1"]
[]
[]
["     C","spare","  -","  -","  -","  -","( 34-way )","BLUE","C-spare",null,"BLUE","C-spare",null,"( 34-way )"]
[]
[]
[]
["     CONTROL  SIGNALS  CABLE  CONNECTORS  AT",{"$nulls":8},"      CONTROL  SIGNALS  CABLE"]
["             PATCHBOX  CONTROL  DRIVER  PCBs",{"$nulls":8},"CONNECTORS AT HELIX DRIVER PCBs"]
[]
["PATCH-","PCB","B/PLANE","TEST-","NOT-","SERIAL","F/PANEL","CABLE","CABLE",null,"CABLE","CABLE",null,"F/PANEL","PCB"]
["BOX","SLOT","CONNEC.","PULSE","RESET","LOAD","CONNEC.","MARKER","LABEL",null,"MARKER","LABEL",null,"CONNEC.","SLOT"]
[{"$nulls":6},"( 34-way )",{"$nulls":6},"( 34-way )"]
[]
["     D","slot 4","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1 ","BLUE","D-4-31",null,"BLUE","16-A-1",null,"     A-1",16]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","D-4-32",null,"BLUE","16-A-2",null,"     A-2"]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","D-4-33",null,"BLUE","16-B-1",null,"     B-1"]
[]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","D-4-34",null,"BLUE","17-A-1",null,"     A-1",17]
[]
[]
["     D","slot 10","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","D-10-31",null,"BLUE","17-A-2",null,"     A-2"]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","D-10-32",null,"BLUE","17-B-1",null,"     B-1"]
[]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","D-10-33",null,"BLUE","18-A-1",null,"     A-1",18]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","D-10-34",null,"BLUE","18-A-2",null,"     A-2"]
[]
[]
["     D","slot 16","P1/1-15","TP(1-5)","RS(1-5)","LD(1-5)","Control-1","BLUE","D-16-31",null,"BLUE","18-B-1",null,"     B-1"]
[]
[null,null,"P1/16-31","TP(6-10)","RS(6-10)","LD(6-10)","Control-2","BLUE","D-16-32",null,"BLUE","19-A-1",null,"     A-1",19]
[]
[null,null,"P2/1-15","TP(11-15)","RS(11-15)","LD(11-15)","Control-3","BLUE","D-16-33",null,"BLUE","19-A-2",null,"     A-2"]
[null,null,"P2/16-31","TP(16-20)","RS(16-20)","LD(16-20)","Control-4","BLUE","D-16-34",null,"BLUE","19-B-1",null,"     B-1"]
[]
[]
["     D","spare","  -","  -","  -","  -","( 34-way )","BLUE","D-spare",null,"BLUE","D-spare",null,"( 34-way )"]