{"text_format":"5","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"props":{"creator":"mp","last_modified_by":"mp","company":"UCL"},"not_rendered":{"external_links":1},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":69,"n_cols":11,"rows_kept":69,"flags":["formulas_cached_only"]}
[]
[]
["LV  SUPPLY CABLE CONNECTORS AT",{"$nulls":6},"LV  SUPPLY CABLE CONNECTORS AT"]
["  PATCHBOX  CLOCK  DRIVER  PCBs",{"$nulls":6},"HELIX DRIVER POWER SUPPLY CRATE"]
[]
["PATCH-","PCB","CONNEC.","F/PANEL","CABLE","CABLE",null,"CABLE","CABLE","CONNEC.","CONNEC."]
["BOX","SLOT","NUMBER","CONNEC.","MARKER","LABEL",null,"MARKER","LABEL","NUMBER","  TYPE"]
[]
["     A","slot   3",null,"9-pin D","RED","   A 3",null,"RED","   A 3",null,"9-pin D"]
[null,"slot   9",null,"9-pin D","RED","   A 9",null,"RED","   A 9",null,"9-pin D"]
[null,"slot   15",null,"9-pin D","RED","   A 15",null,"RED","   A 15",null,"9-pin D"]
[]
["     A","spare",null,"9-pin D","RED","   A 01",null,"RED","   A 01",null,"9-pin D"]
[]
[]
["     B","slot   3",null,"9-pin D","RED","   B 3",null,"RED","   B 3",null,"9-pin D"]
[null,"slot   9",null,"9-pin D","RED","   B 9",null,"RED","   B 9",null,"9-pin D"]
[null,"slot   15",null,"9-pin D","RED","   B 15",null,"RED","   B 15",null,"9-pin D"]
[]
["     B","spare",null,"9-pin D","RED","   B 01",null,"RED","   B 01",null,"9-pin D"]
[]
[]
["     C","slot   3",null,"9-pin D","RED","   C 3",null,"RED","   C 3",null,"9-pin D"]
[null,"slot   9",null,"9-pin D","RED","   C 9",null,"RED","   C 9",null,"9-pin D"]
[null,"slot   15",null,"9-pin D","RED","   C 15",null,"RED","   C 15",null,"9-pin D"]
[]
["     C","spare",null,"9-pin D","RED","   C 01",null,"RED","   C 01",null,"9-pin D"]
[]
[]
["     D","slot   3",null,"9-pin D","RED","   D 3",null,"RED","   D 3",null,"9-pin D"]
[null,"slot   9",null,"9-pin D","RED","   D 9",null,"RED","   D 9",null,"9-pin D"]
[null,"slot   15",null,"9-pin D","RED","   D 15",null,"RED","   D 15",null,"9-pin D"]
[]
["     D","spare",null,"9-pin D","RED","   D 01",null,"RED","   D 01",null,"9-pin D"]
[]
[]
[]
["LV  SUPPLY CABLE CONNECTORS AT",{"$nulls":6},"LV  SUPPLY CABLE CONNECTORS AT"]
["PATCHBOX  CONTROL  DRIVER  PCBs",{"$nulls":6},"HELIX DRIVER POWER SUPPLY CRATE"]
[]
["PATCH-","PCB","CONNEC.","F/PANEL","CABLE","CABLE",null,"CABLE","CABLE","CONNEC.","CONNEC."]
["BOX","SLOT","NUMBER","CONNEC.","MARKER","LABEL",null,"MARKER","LABEL","NUMBER","  TYPE"]
[]
["     A","slot   4",null,"9-pin D","BLUE","   A 4",null,"BLUE","   A 4",null,"9-pin D"]
[null,"slot   10",null,"9-pin D","BLUE","   A 10",null,"BLUE","   A 10",null,"9-pin D"]
[null,"slot   16",null,"9-pin D","BLUE","   A 16",null,"BLUE","   A 16",null,"9-pin D"]
[]
["     A","spare",null,"9-pin D","BLUE","   A 02",null,"BLUE","   A 02",null,"9-pin D"]
[]
[]
["     B","slot   4",null,"9-pin D","BLUE","   B 4",null,"BLUE","   B 4",null,"9-pin D"]
[null,"slot   10",null,"9-pin D","BLUE","   B 10",null,"BLUE","   B 10",null,"9-pin D"]
[null,"slot   16",null,"9-pin D","BLUE","   B 16",null,"BLUE","   B 16",null,"9-pin D"]
[]
["     B","spare",null,"9-pin D","BLUE","   B 02",null,"BLUE","   B 02",null,"9-pin D"]
[]
[]
["     C","slot   4",null,"9-pin D","BLUE","   C 4",null,"BLUE","   C 4",null,"9-pin D"]
[null,"slot   10",null,"9-pin D","BLUE","   C 10",null,"BLUE","   C 10",null,"9-pin D"]
[null,"slot   16",null,"9-pin D","BLUE","   C 16",null,"BLUE","   C 16",null,"9-pin D"]
[]
["     C","spare",null,"9-pin D","BLUE","   C 02",null,"BLUE","   C 02",null,"9-pin D"]
[]
[]
["     D","slot   4",null,"9-pin D","BLUE","   D 4",null,"BLUE","   D 4",null,"9-pin D"]
[null,"slot   10",null,"9-pin D","BLUE","   D 10",null,"BLUE","   D 10",null,"9-pin D"]
[null,"slot   16",null,"9-pin D","BLUE","   D 16",null,"BLUE","   D 16",null,"9-pin D"]
[]
["     D","spare",null,"9-pin D","BLUE","   D 02",null,"BLUE","   D 02",null,"9-pin D"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}