RCAL space, MVD cables and GG magnet RCAL space 200 across x 240mm high

191mm

200mm

GG magnet diameter 180mm

Cable bunches enclosed in zipper tube - 5 combo cables in each barrel set, 4 combo cables in each wheel set, 44 bunches in total. In addition: Radiation monitor cables (red) and sensors (black)

magnet shielding at each corner at REAR inactive part of RCAL

60mm

60mm

largest diameter 192mm is at beampipe outside RCAL, between RTD and RCAL