single dogleg 200 um

one tape 225 + one dogleg 200

two tapes 450 + dogleg 200

three tapes 675 + dogleg 200

four tapes 900 + dogleg 200

five tapes 1125 + dogleg 200

tape width 21mm

distance between insert noses 33mm

425 um

650 um

875 um

1100 um

1325 um nose of insert harness retainer clamp 0.5mm CF or moulded PEEK

assume dogleg 200 microns thick assume one double tape max 225 microns thick

also for

also for

also for

UCL-DH003b ATLAS SCT BARREL HARNESS CLAMP types L, M and H

centre of tape

section across d and e - see UCL-DH003a

bridge for optofibre ribbon or sleeved fibre gap 1.0mm high x 3.5mm across

gap 450

gap 900

gap 1350

CLAMP TYPE: Low

CLAMP TYPE: Medium

CLAMP TYPE: High

gap width 22mm

total width of clamp 36mm

TJF version 01.03.01

18mm um um um