18 single fibres in furcation tubing 0.9mm diam. in one bunch

ATLAS SCT data fibres from one harness - route past last ’dogleg to tape connector’ before end of barrel

TJF 22.03.01

3.48 connector

PCB

5 low mass tapes

0.8

1.31 barrel surface

2.5

6mm

3.48 connector

PCB

5 low mass tapes

0.8

1.31 barrel surface

connector, PCB, tape heights from TW 01.03.01 PCB drawn as extending beyond connector edge

2.5

4.05mm 2.25mm alternative - separate 6 way and 12 way bunches and route either side of connector